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Rating of EXCEPTIONAL
91 - 100 Points

For Surface Appearance
Uniform and consistent throughout in texture. Clean tight longitudinal joints.  Few, if any, fat spots.  Little or no discernable roller marks.
For Smoothness
Consistently smoothness throughout. Smooth transitions at pavement ends or bridges. No significant bumps at transverse joints. No discernable surface irregularities that affect ride, i.e., rutting, roller marks, etc.
Rating of VERY GOOD
80 - 90 Points

For Surface Appearance
Long sections of uniform surface appearance. Isolated areas of minor segregation or surface imperfections. Isolated and minor imperfections in longitudinal joints, i.e. separation, raveling, overlapping, etc.
For Smoothness
Long sections of smoothness.  Isolated areas of minor chatter or uneven surface.  
Minor roughness in transition areas.  Discernable bump at transverse joints.Rating of GOOD
< 80 Points

For Surface Appearance
Random or widely scattered areas of surface imperfections.  Noticeable end-load segregation.  Discernable roller marks or auger shadows are more prevalent.  Noticeable problems with longitudinal joints are more prevalent.
For Smoothness
Surface irregularities (i.e. dips, bumps, chatter, etc.) are more widespread. 
Presence of rutting. Significant roughness in transition areas. Significant bump at transverse joints.
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      For  Surface  Appearance   Uniform and consistent throughout in texture. Clean tight longitudinal joints.    Few, if any, fat  spots.    Little or no discernable roller marks.   For Smoothness   Consistently smooth ness   throughout. Smooth transitions at pavement ends or bridges. No  significant bumps at transverse joints. No discernable surface irregularities that affect ride, i.e.,  rutting, roller marks, etc.     For  Surface Appearance   Long sections of uniform surface appearance. Isolated areas of minor segregation or surface  imperfections. Isolated and minor imperfections in longitudinal joints, i.e. separation, raveling,  overlapping, etc.   For Smoothness   Long sections of smoothness.  Isolated areas of minor chatter or uneven surface.     Minor roughness in transition areas.  Discernable bump at transverse joints.   For  Surface  Appearance   Random or widely scattered  areas of surface imperfections.   N oticeable end - load segregation.   Discernable roller marks or auger shadows are more prevalent.    Noticeable problems with  longitudinal joints are more prevalent.   For Smoothness   Surface irregularities (i.e. dips, bumps, chatter, etc.) are more widespread.    Presence of rutting. Significant roughness in transition areas. Significant bump at transverse  joints.  
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