|  |  |  |  |
| --- | --- | --- | --- |
|  | **Company**  Skyweb Inspection Checklist  *Sign and date inspection and completeness*. *Transfer any punchlist items to open cells, then sign and date when complete*d. | | **Project Name**  **Location**  **Customer/GC** |
| **Description** | **Company Rep (Date)** | **GC Rep (Date)** | **Comments/Punchlist Items?** |
| Perimeter straps installed at correct locations. |  |  |  |
| Correct number of loops hooked at eave |  |  |  |
| Skyweb installed in correct orientation |  |  |  |
| Correct number of loops hooked at gable |  |  |  |
| All splices appear neat and proper |  |  |  |
| No holes or snags in mesh |  |  |  |
| Skyweb tension appears correct |  |  |  |
| Excess skyweb trimmed |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Empresa**  Lista de Verificación de Inspección de Skyweb  Firma y fecha al terminar la inspección. Ingrese cualquier elemento de tareas pendientes a las celdas abiertas, luego ingrese firma y fecha cuando estén completados. | | **Nombre del Proyecto:**  **Ubicación:**  **Cliente/Contratista General:** |
| **Descripción:** | **Representante de Empresa (Fecha):** | **Rep CG (Fecha)** | **Comentarios/Elementos Pendientes** |
| Las correas perimetrales están instaladas en las ubicaciones correctas. |  |  |  |
| El número correcto de bucles está enganchado en el alero. |  |  |  |
| Skyweb está instalado en la orientación correcta. |  |  |  |
| El número correcto de bucles está enganchado en el hastial. |  |  |  |
| Todas las uniones parecen ordenadas y adecuadas. |  |  |  |
| No hay agujeros ni desgarres en la malla. |  |  |  |
| La tensión del Skyweb parece correcta. |  |  |  |
| El exceso de Skyweb ha sido recortado. |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |